Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_coordinate_range Struct Reference

This report is capable of getting the coordinate range from the device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_COORDINATERANGE.
unsigned short | x_min
| Minimum logical value in the horizontal direction to be returned by the device.
unsigned short | x_max
| Maximum logical value in the horizontal direction to be returned by the device.
unsigned short | y_min
| Minimum logical value in the vertical direction to be returned by the device.
unsigned short | y_max
| Maximum logical value in the vertical direction to be returned by the device.

## Detailed Description

This report is capable of getting the coordinate range from the device.

Examples
  example-image-cairo.c, example-image-gdiplus.cpp, and example-reading.c.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h