Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_run_mode Struct Reference

This report is capable of both sending and receiving the current device run mode. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be set to SCRIPTEL_FEATURE_RUNMODE.
scriptel_device_run_mode | run_mode
| Run mode the device is currently in or should be set to.

## Detailed Description

This report is capable of both sending and receiving the current device run mode.

Run modes are defined in the scriptel_device_run_mode enumeration.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h