Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_input_debug_coordinate Struct Reference

This structure contains information about a debug coordinate from a ScripTouch device with debug firmware. More...

`#include <scriptel-hid-reports.h>`

Collaboration diagram for scriptel_hid_input_debug_coordinate:
[legend]

## Data Fields
unsigned char | report_id
| Report ID, should always be set to SCRIPTEL_INPUT_DEBUGCOORDINATE.
scriptel_sample_info | sample_info
| Information about the sample.
unsigned short | offset
| Offset of the coordinate.
unsigned short | x_max
| Maximum horizontal sample.
unsigned short | x_min
| Minimum horizontal sample.
unsigned short | y_max
| Maximum vertical sample.
unsigned short | y_min
| Minimum vertical sample.
unsigned short | x_errcor
| The horizontal coordinate after error correction.
unsigned short | y_errcor
| The vertical coordinate after error correction.
unsigned short | x_mapped
| The horizontal coordinate after being mapped.
unsigned short | y_mapped
| The vertical coordinate after being mapped.
unsigned char | region
| The region the last pen down even occurred in.

## Detailed Description

This structure contains information about a debug coordinate from a ScripTouch device with debug firmware.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h