Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_operating_modes Struct Reference

This report gets the supported operating modes of the device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_OPERATINGMODE.
unsigned char | supported_modes
| Bit mask for supported capture modes, corresponds to scriptel_device_acquisition_mode.
unsigned char | reserved
| Reserved for future use.
unsigned char | acquisition_mode
| Current acquisition mode maps to scriptel_device_acquisition_mode.
unsigned char | touch_mode
| Current touch mode, maps to scriptel_device_pentouch_mode.
unsigned char | pen_mode
| Current pen mode, maps to scriptel_device_pentouch_mode.

## Detailed Description

This report gets the supported operating modes of the device.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h