Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_general_parameters Struct Reference

This report gets and sets general digitizer parameters for the device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, Should always be SCRIPTEL_FEATURE_GENERALPARAMETERS.
unsigned char | xy_output_enable
| Whether or not coordinates are going to be sent.
unsigned char | adc_output_enable
| Whether or not to send ADC output.
unsigned char | map_coordinates
| Whether or not coordinates get mapped to the host range.
unsigned char | channel_lock_enable
| Whether or not to use channel lock mode.
unsigned char | channel_lock_number
| Channel index for channel lock mode.
unsigned char | reserved
| Reserved – currently unused.
unsigned char | corner_lower_left
| Number of the lower left corner.
unsigned char | corner_upper_left
| Number of the upper left corner.
unsigned char | corner_lower_right
| Number of the lower right corner.
unsigned char | corner_upper_right
| Number of the upper right corner.
unsigned short | samples
| Samples.
unsigned char | filter_frequency
| Filter frequency.

## Detailed Description

This report gets and sets general digitizer parameters for the device.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h