Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_serial_number Struct Reference

This report is capable of getting and setting the internal serial number on the device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_SERIALNUMBER.
unsigned char | serial_number [32]
| Serial number is a maximum of 32 unsigned chars. More...
unsigned char | write_key_1
| Write Key 1 - Should be 'S' for writing, cleared when reading.
unsigned char | write_key_2
| Write Key 2 - Should be 'N' for writing, cleared when reading.

## Detailed Description

This report is capable of getting and setting the internal serial number on the device.

## Field Documentation

## ◆ serial_number

unsigned char serial_number[32]

Serial number is a maximum of 32 unsigned chars.

The serial number can be padded with either spaces ' ' (0x20) or NULL (0x00). It's safer to assume there isn't any padding and treat it like binary data. Serial number of the device.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h