Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_device_status Struct Reference

This report contains information about a ScripTouch device's current running state. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should be set to SCRIPTEL_FEATURE_DEVICE_STATUS.
unsigned char | is_initializing
| Is initializing.
unsigned char | is_idle
| Is Idle (command mode)
unsigned char | calibration_required
| Calibration required (is not calibrated)
unsigned char | is_calibrating
| Is calibrating.
unsigned char | all_output_commands_locked
| All output is locked.
unsigned char | operating_mode_commands_locked
| Operating mode commands locked.
unsigned char | region_commands_locked
| Region commands locked.
unsigned char | screen_commands_locked
| Screen commands locked.
unsigned char | display_commands_locked
| Display commands locked.
unsigned char | calibration_commands_locked
| Calibration commands locked.
unsigned char | reserved1
| Reserved for future use.
unsigned short | reserved2
| Reserved for future use.
unsigned short | last_error
| The last error that occured, cleared on power up.
char | error_info [64]
| An human readable string explaining the error.

## Detailed Description

This report contains information about a ScripTouch device's current running state.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h