ProScript .NET Documentation
ProScript .NET Documentation
ProScript
ADCChannelValues Class
ADCScanValues Class
AdjustedCoordinate Class
ButtonDown Class
ButtonEvent Class
ButtonMove Class
ButtonPress Class
ButtonUp Class
CalibrationData Class
CalibrationState Class
Capabilities Class
CardParser Class
Configuration Class
Coordinate Class
CoordinateRange Class
DebugCoordinate Class
Device Class
Device.CoordinateType Enumeration
DeviceManager Class
DeviceProductRestriction Class
DeviceStatus Class
Display Class
DisplayChunk Class
DisplaySettings Class
ExtendedCoordinate Class
FinancialCard Class
FinancialCardIssuer Class
FinancialCardIssuerName Enumeration
FinancialCardTrackOne Class
FinancialCardTrackTwo Class
FirmwarePage Class
FrequencyAmplitude Class
FWFirmwareDevice Class
FWFirmwarePackage Class
FWFirmwarePackageFormat Class
GeneralParameters Class
IdentificationCard Class
IdentificationCardTrackOne Class
IdentificationCardTrackThree Class
IdentificationCardTrackTwo Class
IdentificationSex Enumeration
IDeviceNotificationListener Interface
IFirmwareListener Interface
IFirmwarePackage Interface
IFirmwareRestriction Interface
IInputListener Interface
MagneticCardSwipe Class
OperatingModes Class
OutputConfiguration Class
PenParameters Class
PeripheralConfiguration Class
Region Class
RegionButton Class
RegionContainer Class
RegionGraphic Class
RegionLine Class
RegionNull Class
RegionText Class
Resource Class
ResourceAvailability Class
ResourceGraphic Class
ResourceInfo Class
ResourceInfo.Justification Enumeration
ResourceInfo.ScreenRegionSaveChanges Enumeration
ResourceInfo.Type Enumeration
ResourceInvalid Class
ResourceText Class
Screen Class
ScreenModify Class
ScreenRegionInfo Class
Signature Class
SRECFirmwarePackage Class
SRECParseException Class
SRECRecord Class
STException Class
TouchParameters Class
Version Class

# ProScript Namespace

Classes

| Class | Description
--- | --- | ---
| ADCChannelValues | This class reports ADC channel values from a ScripTouch device.
| ADCScanValues | This class represents an ADC scan value sample from a ScripTouch device.
| AdjustedCoordinate | This class represents a coordinate that has been adjusted for range and aspect.
| ButtonDown | This class represents a button down event from a ScripTouch device.
| ButtonEvent | This class represents an abstract button event
| ButtonMove | This class represents a button press event from a ScripTouch device.
| ButtonPress | This class represents a button press event from a ScripTouch device.
| ButtonUp | This class represents a button down event from a ScripTouch device.
| CalibrationData | This class represents calibration parameters of a ScripTouch device. It is used for internal Scriptel engineering and development as well as to support the desire to save calibration data and restore the same calibration data back at a later time. This can be accomplished through getJSONCalibrationBlob() and the String constructor respectively.
| CalibrationState | This class represents the current calibration state of the device.
| Capabilities | This class represents the physical capabilities of a ScripTouch device
| CardParser | This class is a static helper class used to help parse Magnetic Swipe cards.
| Configuration | This class represents the device configuration on a ScripTouch mouse device.
| Coordinate | This class represents a basic coordinate coming from a ScripTouch device.
| CoordinateRange | This class represents the logical coordinate range of a ScripTouch device.
| DebugCoordinate | This class represents a coordinate coming from a debug build of firmware for a ScripTouch device.
| Device | This class represents a physical ScripTouch device.
| DeviceManager | This class manages ScripTouch devices.
| DeviceProductRestriction | This class is used to check if a device has the proper product id for the target firmware.
| DeviceStatus | This class represents output parameters of a ScripTouch device.
| Display | This class contains static information regarding the display of a ScripTouch device.
| DisplayChunk | This class represents an image raster that can be transferred to the display on a ScripTouch device.
| DisplaySettings | This class represents dynamic display options that can be changed.
| ExtendedCoordinate | This class represents an extended coordinate coming from a ScripTouch device.
| FinancialCard | This class represents the parsed magnetic stripe data from a financial (credit) card. See "http://en.wikipedia.org/wiki/Magnetic_stripe_card">http://en.wikipedia.org/wiki/Magnetic_stripe_card
| FinancialCardIssuer | This class attempts to identify credit card issuers based on patterns in the numbers each vendor issues.
| FinancialCardTrackOne | This class represents track one of a financial card.
| FinancialCardTrackTwo | This class represents the second track of a financial card
| FirmwarePage | This class represents a page of firmware that can be written to the device.
| FrequencyAmplitude | This class represents frequency and amplitude settings for a ScripTouch device.
| FWFirmwareDevice | This class represents a device that the firmware is allowed to be placed on.
| FWFirmwarePackage | This class contains the information needed to properly download firmware from a .FW firmware file
| FWFirmwarePackageFormat | This class represents a complete firmware package
| GeneralParameters | This class represents general operating parameters for a ScripTouch device.
| IdentificationCard | This class represents an identification card such as a United States drivers license. http://www.aamva.org/?aspxerrorpath=/NR/rdonlyres/66260AD6-64B9-45E9-A253-B8AA32241BE0/0/2005DLIDCardSpecV2FINAL.pdf
| IdentificationCardTrackOne | This class represents track one of the magnetic strip of an identification card, such as a United States drivers license.
| IdentificationCardTrackThree | This class represents track three of a magnetic strip identification card such as a United States driver's license.
| IdentificationCardTrackTwo | This class represents track two of a magnetic strip identification card such as a United States driver's license.
| MagneticCardSwipe | This class represents a swipe of a magnetic swipe card on an equipped ScripTouch device.
| OperatingModes | The class represents compatible operating modes of a ScripTouch device.
| OutputConfiguration | This class represents output parameters of a ScripTouch device.
| PenParameters | This class represents pen parameters of a ScripTouch device.
| PeripheralConfiguration | This class represents the peripheral parameters of a ScripTouch device.
| Region | This class represents a region. A region is a box shaped object stored in the memory of a ScripTouch device that can take several forms such as lines, buttons, and containers.
| RegionButton | This class represents a button region.
| RegionContainer | This class represents a container region in a ScripTouch device.
| RegionGraphic | This class represents a graphic region on the device.
| RegionLine | This class represents a line region in a ScripTouch device.
| RegionNull | This class represents a line region in a ScripTouch device.
| RegionText | This class represents a text region on the device.
| Resource | This class represents a resource. A resource is an image or character set that is always commited to memory due to the large possible size of a resource.
| ResourceAvailability | This class represents the amount of space available for resources.
| ResourceGraphic | This class represents a graphic resource stored on the device.
| ResourceInfo | This class represents the information about a resource.
| ResourceInvalid | This class represents a null or invalid resource.
| ResourceText | This class represents a text resource.
| Screen | This class represents a screen.
| ScreenModify | This class represents a message that modifies a screen on the device.
| ScreenRegionInfo | This class represents screen and region limitations of a ScripTouch device.
| Signature | This class represents a signature. As signature points are received from the device, they can be added to a Signature object to track signature strokes, as well as to render the signature as an Image.
| SRECFirmwarePackage | This class can be used to read Motorola SRecord files produced by most of the Renesas tools.
| SRECParseException | This exception represents some problem reading an SREC file.
| SRECRecord | This represents a single line in the SREC file which represents part of the overall program structure.
| STException | This class represents an Exception that can be thrown for various errors related to communication with a ScripTouch device
| TouchParameters | This class represents touch parameters in a ScripTouch device.
| Version | This class represents the firmware version of a ScripTouch device.

Interfaces

| Interface | Description
--- | --- | ---
| IDeviceNotificationListener | This interface is used to describe a class that is capable of receiving hot plug notifications from DeviceManager.
| IFirmwareListener | This interface is used to receive firmware update percentage notifications.
| IFirmwarePackage | This interface is used to define a type of class that can be used for reading firmware files for the ScripTouch series of devices.
| IFirmwareRestriction | This interface is used to define an abstract firmware download restriction. Firmware restrictions are used by firmware packages to introduce requirements that must be met in order to download that firmware.
| IInputListener | This interface describes a class capable of receiving input events from a ScripTouch device.

Enumerations

| Enumeration | Description
--- | --- | ---
| Device CoordinateType | Defines the coordinate system used for simulating pen touches
| FinancialCardIssuerName | Enumeration containing known financial card issuers.
| IdentificationSex | This class represents the gender of a card-holder on an identification card.
| ResourceInfo Justification | This enumeration contains the different types of justifications that can be applied to either a GRAPHIC or TEXT.
| ResourceInfo ScreenRegionSaveChanges | This enumeration contains valid screen region save states.
| ResourceInfo Type | This enumeration contains all valid resource types and their numeric identifiers.

Copyright 2015 Scriptel Corporation. All Rights Reserved.