ProScript .NET Documentation
ProScript .NET Documentation
ProScript
Capabilities Class
Capabilities Fields
CardReaderHid Field
CardReaderInterchangeable Field
CardReaderKeyboardBasic Field
CardReaderKeyboardPreamble Field
CardReaderNone Field
CoordinateSupportsBuffering Field
CoordinateSupportsCompression Field
CoordinateSupportsStreaming Field
CoordinateSupportsThrottling Field
DisplayType240x64and1x5BlackWhite Field
DisplayType240x64and1x5GrayScale Field
DisplayTypeNone Field
MagCardReaderChangeable Field
MagCardReaderHID Field
MagCardReaderKeyboard Field
SupportedReportsHid Field
SupportedReportsKeyboard Field
SupportedReportsMouse Field
SupportedReportsPen Field
SupportedReportsTouch Field

# Capabilities Fields

The Capabilities type exposes the following members.

Fields

| Name | Description
--- | --- | ---
| CardReaderHid | Obsolete. The device has a card reader that supports Scriptel HID reports.
| CardReaderInterchangeable | Obsolete. The device has a card reader that is capable of switching between Keyboard output and Scriptel HID reports.
| CardReaderKeyboardBasic | Obsolete. The device has a card reader that supports HID keyboard reports.
| CardReaderKeyboardPreamble | Obsolete. The device has a card reader that supports HID keyboard reports with a Scriptel preamble.
| CardReaderNone | Obsolete. The device has no card reader.
| CoordinateSupportsBuffering | The device supports buffering coordinates.
| CoordinateSupportsCompression | The device supports compression.
| CoordinateSupportsStreaming | The device supports streaming coordinates.
| CoordinateSupportsThrottling | The device supports throttling.
| DisplayType240x64and1x5BlackWhite | The device has a 240x64 pixel display that is 1x5 inches and is black and white.
| DisplayType240x64and1x5GrayScale | The device has a 240x64 pixel display that is 1x5 inches and is grayscale.
| DisplayTypeNone | The device does not have a display.
| MagCardReaderChangeable | The device has an equipped magnetic strip reader that can change between HID reports and keyboard events.
| MagCardReaderHID | The device has an equipped magnetic strip reader that will output swipes to vendor-specific HID.
| MagCardReaderKeyboard | The device has an equipped magnetic strip reader that will output swipes to raw keyboard events.
| SupportedReportsHid | The device supports Scriptel HID reports.
| SupportedReportsKeyboard | The device supports HID keyboard reports.
| SupportedReportsMouse | The device supports HID mouse reports.
| SupportedReportsPen | The device supports HID digitizer reports.
| SupportedReportsTouch | The device supports HID touch reports.

Top
See Also

#### Reference

Capabilities Class
ProScript Namespace

Copyright 2015 Scriptel Corporation. All Rights Reserved.