ProScript .NET Documentation
ProScript .NET Documentation
ProScript
Capabilities Class
Capabilities Constructor
Capabilities Methods
Capabilities Fields

# Capabilities Class

This class represents the physical capabilities of a ScripTouch device
Inheritance Hierarchy
System
Object
ProScript
Capabilities

Namespace: ProScript
Assembly: proscript-csharp (in proscript-csharp.dll) Version: 1.6.39.0 (1.6.39.0)
Syntax
C#
VB
C++
F#
Copy

    public class Capabilities

    Public Class Capabilities

    public ref class Capabilities

    type Capabilities =  class end

The Capabilities type exposes the following members.

Constructors

| Name | Description
--- | --- | ---
| Capabilities | Initializes a new instance of the Capabilities class.

Top
Methods

| Name | Description
--- | --- | ---
| Equals | Determines whether the specified Object is equal to the current Object. (Inherited from Object.)
| GetBrightnessLevels | Gets the number of brightness levels supported.
| GetCalibrationXMax | The maximum x value of the firmware's internal mapping space
| GetCalibrationXMin | The minimum x value of the firmware's internal mapping space
| GetCalibrationYMax | The maximum y value of the firmware's internal mapping space
| GetCalibrationYMin | The minimum y value of the firmware's internal mapping space
| GetCardReader | Gets the type of card reader equipped on this device.
| GetColorDepth | Gets the bit depth of the display.
| GetContrastLevels | Gets the number of contrast levels supported.
| GetCoordinateModes | The coordinate modes supported by the device.
| GetCoordinateXMax | Gets the maximum X coordinate.
| GetCoordinateXMin | Gets the minimum X coordinate.
| GetCoordinateYMax | Gets the maximum Y coordinate.
| GetCoordinateYMin | Gets the minimum Y coordinate.
| GetDigitizerHeight | Gets the height of the digitizer in millimeters.
| GetDigitizerWidth | Gets the width of the digitizer in millimeters.
| GetDisplayHeight | Gets the height of the display in pixels.
| GetDisplayId | Gets the type of display contained in this device. 0 = None 1 = 240x64, binary 2 = 240x64, 16 gray
| GetDisplayWidth | Gets the width of the display in pixels.
| GetHashCode | Serves as a hash function for a particular type. (Inherited from Object.)
| GetReserved10 | The parameter is not used.
| GetReserved11 | The parameter is not used.
| GetReserved12 | The parameter is not used.
| GetReserved13 | The parameter is not used.
| GetReserved14 | The parameter is not used.
| GetReserved4 | The parameter is not used.
| GetReserved5 | The parameter is not used.
| GetReserved6 | The parameter is not used.
| GetReserved7 | The parameter is not used.
| GetReserved9 | The parameter is not used.
| GetSupportedReports | Gets a bit mask containing report types this device supports.
| GetSupportsScreensResources | Returns whether this device is capable of using screen and resource calls.
| GetType | Gets the type of the current instance. (Inherited from Object.)
| ToString | Converts this object into a human readable string. (Overrides Object ToString .)

Top
Fields

| Name | Description
--- | --- | ---
| CardReaderHid | Obsolete. The device has a card reader that supports Scriptel HID reports.
| CardReaderInterchangeable | Obsolete. The device has a card reader that is capable of switching between Keyboard output and Scriptel HID reports.
| CardReaderKeyboardBasic | Obsolete. The device has a card reader that supports HID keyboard reports.
| CardReaderKeyboardPreamble | Obsolete. The device has a card reader that supports HID keyboard reports with a Scriptel preamble.
| CardReaderNone | Obsolete. The device has no card reader.
| CoordinateSupportsBuffering | The device supports buffering coordinates.
| CoordinateSupportsCompression | The device supports compression.
| CoordinateSupportsStreaming | The device supports streaming coordinates.
| CoordinateSupportsThrottling | The device supports throttling.
| DisplayType240x64and1x5BlackWhite | The device has a 240x64 pixel display that is 1x5 inches and is black and white.
| DisplayType240x64and1x5GrayScale | The device has a 240x64 pixel display that is 1x5 inches and is grayscale.
| DisplayTypeNone | The device does not have a display.
| MagCardReaderChangeable | The device has an equipped magnetic strip reader that can change between HID reports and keyboard events.
| MagCardReaderHID | The device has an equipped magnetic strip reader that will output swipes to vendor-specific HID.
| MagCardReaderKeyboard | The device has an equipped magnetic strip reader that will output swipes to raw keyboard events.
| SupportedReportsHid | The device supports Scriptel HID reports.
| SupportedReportsKeyboard | The device supports HID keyboard reports.
| SupportedReportsMouse | The device supports HID mouse reports.
| SupportedReportsPen | The device supports HID digitizer reports.
| SupportedReportsTouch | The device supports HID touch reports.

Top
See Also

#### Reference

ProScript Namespace

Copyright 2015 Scriptel Corporation. All Rights Reserved.