# Constant Field Values

## Contents

- com.scriptel.*

## com.scriptel.*

- com.scriptel.proscript.CalibrationState
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `POINT_CENTER` | `0`
  `public static final int` | `POINT_LOWER_LEFT` | `4`
  `public static final int` | `POINT_LOWER_RIGHT` | `6`
  `public static final int` | `POINT_UPPER_LEFT` | `2`
  `public static final int` | `POINT_UPPER_RIGHT` | `8`

- com.scriptel.proscript.Capabilities
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DISPLAY_TYPE_240X64_1X5_BLACKWHITE` | `1`
  `public static final int` | `DISPLAY_TYPE_240X64_1X5_GRAYSCALE` | `2`
  `public static final int` | `DISPLAY_TYPE_NONE` | `0`
  `public static final int` | `SCRIPTEL_CARDREADER_HID` | `1`
  `public static final int` | `SCRIPTEL_CARDREADER_INTERCHANGEABLE` | `131`
  `public static final int` | `SCRIPTEL_CARDREADER_KEYBOARD_BASIC` | `2`
  `public static final int` | `SCRIPTEL_CARDREADER_KEYBOARD_PREAMBLE` | `3`
  `public static final int` | `SCRIPTEL_CARDREADER_NONE` | `0`
  `public static final int` | `SCRIPTEL_MAG_CARDREADER_CHANGEABLE` | `128`
  `public static final int` | `SCRIPTEL_MAG_CARDREADER_HID` | `1`
  `public static final int` | `SCRIPTEL_MAG_CARDREADER_KEYBOARD` | `2`
  `public static final int` | `SUPPORTED_BUFFERING` | `2`
  `public static final int` | `SUPPORTED_COMPRESSION` | `4`
  `public static final int` | `SUPPORTED_REPORTS_HID` | `1`
  `public static final int` | `SUPPORTED_REPORTS_KEYBOARD` | `16`
  `public static final int` | `SUPPORTED_REPORTS_MOUSE` | `2`
  `public static final int` | `SUPPORTED_REPORTS_PEN` | `4`
  `public static final int` | `SUPPORTED_REPORTS_TOUCH` | `8`
  `public static final int` | `SUPPORTED_STREAMING` | `1`
  `public static final int` | `SUPPORTED_THROTTLING` | `8`

- com.scriptel.proscript.Device
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DEVICE_DISCARD_CHANGES` | `0`
  `public static final int` | `DEVICE_FACTORY_RESET` | `90`
  `public static final int` | `DEVICE_SAVE_CHANGES` | `1`
  `public static final int` | `POWER_STATE_NORMAL` | `0`
  `public static final int` | `POWER_STATE_POWERDOWN` | `1`
  `public static final int` | `POWER_STATE_STANDBY` | `2`
  `public static final int` | `RUNMODE_AUTOTOUCH` | `4`
  `public static final int` | `RUNMODE_COMMAND` | `0`
  `public static final int` | `RUNMODE_PEN` | `2`
  `public static final int` | `RUNMODE_PENCONTINUOUS` | `20`
  `public static final int` | `RUNMODE_PENSINGLE` | `16`
  `public static final int` | `RUNMODE_PENSTREAM` | `18`
  `public static final int` | `RUNMODE_TOUCH` | `1`
  `public static final int` | `RUNMODE_TOUCHSINGLE` | `8`
  `public static final int` | `RUNMODE_TOUCHSTREAM` | `10`
  `public static final int` | `SIMULATE_COORD_DEVICE_SPACE` | `2`
  `public static final int` | `SIMULATE_COORD_DISPLAY_SPACE` | `1`
  `public static final int` | `TEXTALIGN_CENTER` | `2`
  `public static final int` | `TEXTALIGN_LEFT` | `0`
  `public static final int` | `TEXTALIGN_RIGHT` | `1`

- com.scriptel.proscript.DisplaySettings
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `SET_COMMAND_COMMIT` | `1`
  `public static final int` | `SET_COMMAND_RESTORE_DEFAULTS` | `128`

- com.scriptel.proscript.FirmwarePage
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `PAGE_SIZE` | `128`

- com.scriptel.proscript.OperatingModes
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ACQMODE_AUTOTOUCH` | `2`
  `public static final int` | `ACQMODE_PEN` | `1`
  `public static final int` | `ACQMODE_TOUCH` | `0`
  `public static final int` | `MODE_CONTINUOUS` | `4`
  `public static final int` | `MODE_SINGLE` | `0`
  `public static final int` | `MODE_SINGLE_LIFTOFF` | `1`
  `public static final int` | `MODE_STREAM` | `2`
  `public static final int` | `MODE_STREAM_LIFTOFF` | `3`

- com.scriptel.proscript.OutputConfiguration
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `COMPRESSION_MODE_HIRES_COMPRESSED` | `3`
  `public static final int` | `COMPRESSION_MODE_HIRES_UNCOMPRESSED` | `2`
  `public static final int` | `COMPRESSION_MODE_LORES_COMPRESSED` | `1`
  `public static final int` | `COMPRESSION_MODE_LORES_UNCOMPRESSED` | `0`
  `public static final long` | `OUTPUT_CONFIGURATION_DEBUG_DATA` | `-2147483648L`
  `public static final long` | `OUTPUT_CONFIGURATION_KEYBOARD` | `65536L`
  `public static final long` | `OUTPUT_CONFIGURATION_MOUSE` | `256L`
  `public static final long` | `OUTPUT_CONFIGURATION_OEM` | `1L`
  `public static final long` | `OUTPUT_CONFIGURATION_OEM_EXTENDED` | `2L`
  `public static final long` | `OUTPUT_CONFIGURATION_PEN_DIGITIZER` | `512L`
  `public static final long` | `OUTPUT_CONFIGURATION_RAW_DATA` | `1073741824L`
  `public static final long` | `OUTPUT_CONFIGURATION_TOUCH` | `1024L`
  `public static final int` | `OUTPUT_MODE_ON_CONFIRM` | `1`
  `public static final int` | `OUTPUT_MODE_ON_HOST_COMMAND` | `2`
  `public static final int` | `OUTPUT_MODE_REALTIME` | `0`

- com.scriptel.proscript.PeripheralConfiguration
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `MAG_CARD_CONFIGURATION_KEYBOARD` | `4`
  `public static final int` | `MAG_CARD_CONFIGURATION_KEYBOARD_PREAMBLE` | `8`
  `public static final int` | `MAG_CARD_CONFIGURATION_OEM_EXTENDED` | `1`

- com.scriptel.proscript.RegionGraphic
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `JUSTIFY_BOTTOM` | `1`
  `public static final int` | `JUSTIFY_CENTER` | `8`
  `public static final int` | `JUSTIFY_LEFT` | `0`
  `public static final int` | `JUSTIFY_RIGHT` | `1`
  `public static final int` | `JUSTIFY_TOP` | `0`

- com.scriptel.proscript.RegionText
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `JUSTIFY_BOTTOM` | `1`
  `public static final int` | `JUSTIFY_CENTER` | `8`
  `public static final int` | `JUSTIFY_LEFT` | `0`
  `public static final int` | `JUSTIFY_RIGHT` | `1`
  `public static final int` | `JUSTIFY_TOP` | `0`

- com.scriptel.proscript.ResourceInfo
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `GRAPHIC` | `1`
  `public static final int` | `INVALID` | `2`
  `public static final int` | `TEXT` | `0`

- com.scriptel.proscript.Screen
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DO_NOTHING_ON_NEXT` | `255`

- com.scriptel.proscript.TuningStatus
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `LOCATION_1_STYLUS_DOWN` | `0`
  `public static final int` | `LOCATION_1_STYLUS_UP` | `1`
  `public static final int` | `LOCATION_2_STYLUS_DOWN` | `2`
  `public static final int` | `LOCATION_2_STYLUS_UP` | `3`

- com.scriptel.proscript.firmware.SRECRecord
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final byte` | `TYPE_BLOCK_HEADER` | `0`
  `public static final byte` | `TYPE_DATA_SEQ_16_BIT` | `1`
  `public static final byte` | `TYPE_DATA_SEQ_24_BIT` | `2`
  `public static final byte` | `TYPE_DATA_SEQ_32_BIT` | `3`
  `public static final byte` | `TYPE_END_OF_BLOCK_16_BIT` | `9`
  `public static final byte` | `TYPE_END_OF_BLOCK_24_BIT` | `8`
  `public static final byte` | `TYPE_END_OF_BLOCK_32_BIT` | `7`
  `public static final byte` | `TYPE_RECORD_COUNT` | `5`

- com.scriptel.proscript.input.MagneticCardSwipe
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `CARD_FORMAT_FINANCIAL` | `1`
  `public static final int` | `CARD_FORMAT_IDENTITY` | `2`
  `public static final int` | `CARD_FORMAT_UNKNOWN` | `255`
  `public static final int` | `TRACK_STATUS_CORRUPT` | `17`
  `public static final int` | `TRACK_STATUS_PARITY_ERROR` | `1`
  `public static final int` | `TRACK_STATUS_UNKNOWN_FORMAT` | `16`
  `public static final int` | `TRACK_STATUS_VALID` | `0`