A B C D E F G H I J L M N O P R S T U V W
All Classes All Packages

## O

open() - Method in class com.scriptel.proscript.Device
  This method attempts to open the device with the operating system.
OperatingModes - Class in com.scriptel.proscript
  The class represents compatible operating modes of a ScripTouch device.
OUTPUT_CONFIGURATION_DEBUG_DATA - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration sending debug data.
OUTPUT_CONFIGURATION_KEYBOARD - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using device as a keyboard.
OUTPUT_CONFIGURATION_MOUSE - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using device as a mouse cursor.
OUTPUT_CONFIGURATION_OEM - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using vender specific output.
OUTPUT_CONFIGURATION_OEM_EXTENDED - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using vender specific output with extended data.
OUTPUT_CONFIGURATION_PEN_DIGITIZER - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using device as a pen digitizer.
OUTPUT_CONFIGURATION_RAW_DATA - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration sending raw signature data.
OUTPUT_CONFIGURATION_TOUCH - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output configuration using device with touch input.
OUTPUT_MODE_ON_CONFIRM - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output mode where coordinates are sent on confirm (usually by pressing "OK").
OUTPUT_MODE_ON_HOST_COMMAND - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output mode where coordinates are buffered until a command from the host.
OUTPUT_MODE_REALTIME - Static variable in class com.scriptel.proscript.OutputConfiguration
  Output mode where coordinates are sent in real time as they're captured.
OutputConfiguration - Class in com.scriptel.proscript
  This class represents output parameters of a ScripTouch device.
OutputConfiguration() - Constructor for class com.scriptel.proscript.OutputConfiguration
  Default constructor which can be used to set the output configuration without first reading it.

A B C D E F G H I J L M N O P R S T U V W
All Classes All Packages