A B C D E F G H I J L M N O P R S T U V W
All Classes All Packages

## M

MAG_CARD_CONFIGURATION_KEYBOARD - Static variable in class com.scriptel.proscript.PeripheralConfiguration
  Mag strip configuration using device as a keyboard.
MAG_CARD_CONFIGURATION_KEYBOARD_PREAMBLE - Static variable in class com.scriptel.proscript.PeripheralConfiguration
  Mag strip configuration using device as a keyboard.
MAG_CARD_CONFIGURATION_OEM_EXTENDED - Static variable in class com.scriptel.proscript.PeripheralConfiguration
  Mag strip configuration using vender specific output.
MagneticCardSwipe - Class in com.scriptel.proscript.input
  This class represents a swipe of a magnetic swipe card on an equipped ScripTouch device.
main(String[]) - Static method in class com.scriptel.proscript.Test
MALE - com.scriptel.proscript.cardswipe.IdentificationSex
mapCoordinates() - Method in class com.scriptel.proscript.GeneralParameters
  Are coordinates being mapped?
MASTER_CARD - com.scriptel.proscript.cardswipe.FinancialCardIssuer
meetsRestriction(Device) - Method in class com.scriptel.proscript.firmware.DeviceProductRestriction
meetsRestriction(Device) - Method in interface com.scriptel.proscript.firmware.FirmwareRestriction
  This will be called by the firmware downloading functions.
MODE_CONTINUOUS - Static variable in class com.scriptel.proscript.OperatingModes
  Mode continuous.
MODE_SINGLE - Static variable in class com.scriptel.proscript.OperatingModes
  Mode single.
MODE_SINGLE_LIFTOFF - Static variable in class com.scriptel.proscript.OperatingModes
  Mode single liftoff.
MODE_STREAM - Static variable in class com.scriptel.proscript.OperatingModes
  Mode stream.
MODE_STREAM_LIFTOFF - Static variable in class com.scriptel.proscript.OperatingModes
  Mode stream liftoff.
modifyScreen(ScreenModify) - Method in class com.scriptel.proscript.Device
  This method is an alternative way to set variables on a screen.

A B C D E F G H I J L M N O P R S T U V W
All Classes All Packages