| EasyScript C API 3.5.29 Platform Independent C Library for EasyScript ScripTouch Devices

Data Fields
scriptel_signature Struct Reference

This structure represents a signature which is made up up the header information as well as zero or more strokes. More...

`#include <scriptel-easyscript.h>`

Collaboration diagram for scriptel_signature:
[legend]

## Data Fields
char * | protocol_version
| The protocol version used to encode/decode this signature. More...
char * | model
| The model number of the device used to make this signature. More...
char * | version
| The firmware version of the device used to make this firmware. More...
int | length
| The number of strokes in this signature. More...
scriptel_stroke * | strokes
| Pointer to the first stroke in the signature. More...
int | width
| Virtual width of the coordinate space (maximum x coordinate). More...
int | height
| Virtual height of the coordinate space (maximum y coordinate). More...

## Detailed Description

This structure represents a signature which is made up up the header information as well as zero or more strokes.

## Field Documentation

## ◆ height

int height

Virtual height of the coordinate space (maximum y coordinate).

## ◆ length

int length

The number of strokes in this signature.

## ◆ model

char* model

The model number of the device used to make this signature.

## ◆ protocol_version

char* protocol_version

The protocol version used to encode/decode this signature.

## ◆ strokes

scriptel_stroke* strokes

Pointer to the first stroke in the signature.

## ◆ version

char* version

The firmware version of the device used to make this firmware.

## ◆ width

int width

Virtual width of the coordinate space (maximum x coordinate).

The documentation for this struct was generated from the following file:

- src/scriptel-easyscript.h