Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_version Struct Reference

This report is capable of getting the device version information. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_VERSIONINFO.
unsigned char | kernel_version [3]
| Kernel version, defunct value, new firmware has this always the same as firmware version. More...
unsigned char | firmware_version [3]
| Version of the installed firmware. More...
unsigned short | asic_signature
| Signature of the ASIC.

## Detailed Description

This report is capable of getting the device version information.

## Field Documentation

## ◆ firmware_version

unsigned char firmware_version[3]

Version of the installed firmware.

Encoded in Binary Coded Decimal.

## ◆ kernel_version

unsigned char kernel_version[3]

Kernel version, defunct value, new firmware has this always the same as firmware version.

Encoded in Binary Coded Decimal.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h