Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_display_chunk Struct Reference

This structure contains information about a raster that should be displayed on the screen of a device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_UPDATEDISPLAYCHUNK.
unsigned short | x
| Where the bitmap should be positioned horizontally.
unsigned short | y
| Where the bitmap should be positioned vertically.
unsigned short | width
| The width of the raster in pixels.
unsigned short | height
| The height of the raster in pixels.
unsigned char | bits_per_pixel
| The number of bits per pixel, 1 for black and white, 4 for monochrome.
unsigned char | graphic [2039]
| This contains the raw raster. More...

## Detailed Description

This structure contains information about a raster that should be displayed on the screen of a device.

## Field Documentation

## ◆ graphic

unsigned char graphic[2039]

This contains the raw raster.

The image should be encoded such that each pixel is encoded with the same width as defined in bits_per_pixel. The image should start with the top left corner and end with the bottom right.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h