Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_asic_reset Struct Reference

This structure allows the reset of a device ASIC. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should be set to SCRIPTEL_FEATURE_ASICRESET.
unsigned char | hardware_reset
| Indicates whether or not a hardware reset (1) or software reset(0) should be used.
unsigned char | reserved
| Reserved for later use.

## Detailed Description

This structure allows the reset of a device ASIC.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h