Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_peripheral_configuration Struct Reference

This structure contains information about peripheral configuration. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should be set to SCRIPTEL_FEATURE_PERIPHERAL_CONFIGURATION.
scriptel_mag_card_output | mag_card_output
| The output mode used by the peripherals, see scriptel_peripheral_output.
unsigned char | reserved1
| Reserved for future use.
unsigned char | reserved2
| Reserved for future use.
unsigned char | reserved3
| Reserved for future use.
unsigned char | reserved4
| Reserved for future use.
unsigned char | reserved5
| Reserved for future use.
unsigned char | reserved6
| Reserved for future use.
unsigned char | reserved7
| Reserved for future use.
unsigned char | reserved8
| Reserved for future use.
unsigned char | reserved9
| Reserved for future use.
unsigned char | reserved10
| Reserved for future use.
unsigned char | reserved11
| Reserved for future use.
unsigned char | reserved12
| Reserved for future use.
unsigned char | reserved13
| Reserved for future use.
unsigned char | reserved14
| Reserved for future use.
unsigned char | save_as_default
| SaveAsDefault.
unsigned char | load_factory_settings
| Load Factory Settings.

## Detailed Description

This structure contains information about peripheral configuration.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h