Scriptel ScripTouch ProScript C Library This documentation contains information about the ScripTouch ProScript C Library.

Data Fields
scriptel_hid_feature_guid Struct Reference

16 byte char array holding the guid value for the device. More...

`#include <scriptel-hid-reports.h>`

## Data Fields
unsigned char | report_id
| Report ID, should always be SCRIPTEL_FEATURE_GENII_CONFIGURATION_AND_DIAGNOSTICS.
unsigned char | guid [16]
| Value of the GUID.

## Detailed Description

16 byte char array holding the guid value for the device.

This is new for ASICless/genII devices.

The documentation for this struct was generated from the following file:

- src/scriptel-hid-reports.h