| EasyScript C API 3.5.29 Platform Independent C Library for EasyScript ScripTouch Devices

Data Fields
scriptel_signature_protocol Struct Reference

This structure contains information about a signature protocol that can be used to decode a signature buffer. More...

`#include <scriptel-easyscript.h>`

## Data Fields
const char * | protocol_name
char | start_stream
char | end_stream
char | cancel
char | pen_up
const char * | sentinel
int | width
int | height
const char | value_table [2][2][23]

## Detailed Description

This structure contains information about a signature protocol that can be used to decode a signature buffer.

## Field Documentation

## ◆ cancel

char cancel

A single character representing that the signature has been cancelled.

## ◆ end_stream

char end_stream

A single character representing the end of stream.

## ◆ height

int height

The logical height of the protocol, used to maintain the aspect ratio of the signature.

## ◆ pen_up

char pen_up

A single character representing pen up events or breaks between strokes.

## ◆ protocol_name

const char* protocol_name

A textual name for the protocol.

## ◆ sentinel

const char* sentinel

A set of characters representing a sentinel that appears immediately after the start of stream character.

## ◆ start_stream

char start_stream

A single character representing the start of stream.

## ◆ value_table

const char value_table[2][2][23]

The value table used to decode the signature.

## ◆ width

int width

The logical width of the protocol, used to maintain the aspect ratio of the signature.

The documentation for this struct was generated from the following file:

- src/scriptel-easyscript.h