# SignatureProtocol

Extends

This interface represents a Scriptel ScripTouch EasyScript protocol.

package | Application

### Methods

## This method should return the character that denotes the signature has been canceled.

    getCancel() : mixed

### Response

`mixed`

## This method should return the character that denotes the end of a stream.

    getEndStream() : mixed

### Response

`mixed`

## This method should return the Height of the device's display in pixels.

    getHeight() : mixed

### Response

`mixed`

## This method should return the character that denotes a "pen up" event, or the start of a new stroke.

    getPenUp() : mixed

### Response

`mixed`

## This method should return the "sentinel" for the stream, the set of characters immediately following the start character.

    getSentinel() : mixed

### Response

`mixed`

## This method should return the character that denotes the start of a new signature.

    getStartStream() : mixed

### Response

`mixed`

## This method should return the width of the device's display in pixels.

    getWidth() : mixed

### Response

`mixed`

## This method should return a two dimensional array containing the values for the high and low x bytes.

    getXValues() : mixed

### Response

`mixed`

## his method should return a two dimensional array containing the values for the high and low y bytes.

    getYValues() : mixed

### Response

`mixed`